QUARTERLY EQUIPMENT MAINTENANCE CHECKLIST:

1. Check filters on compressor and central vacuum.
2. Check compressor oil (if oil-lubricated).
3. Check tubing on delivery systems, nitrous, and vacuum as well as handpiece gaskets and/or coupler O-rings for signs of wear.
4. Clean model trimmer wheel and drain lines.
5. Check hydraulic fluid of patient chair.
6. Check life of computer battery backup (UPS).
7. Test smoke alarms.
8. Verify computer backup by restoring from a backup.